* LED on wrong side of board.
* SD Card on wrong side of board.
* Magenc3 uses PC14 for DO and PC15 CLK. However, these pins are needed for the LSE. One can use multiple CSn pins to talk to multiple mag encoders instead.